①Explanation of the issue regarding the inability to use DFU mode:

1. Check if the module is connected to the computer and inspect the USB cable.

②If not connected, please install the corresponding software driver.

1. Open the folder: Testing Tools—PC Serial Assistant—open the website in the file—download—PC test tools.zip—open CH341SER drive.EXE—install the driver.

2.http://en.szdx-smart.com/EN/zlxz/Development%20tools/PC%20serial%20port%20assistant/303.html—You can directly download PC test tools.zip from our official website and install the driver.

③Programming test:

1. Open the folder: Testing Tools—STM32F103 burning tool—mcuisp.exe—refer to the settings below—after setting, you can perform the programming test.

